USB device details
PixArt Imaging Inc. USB2.0_Camera - Dispositivo compuesto USB

File:  \??\USB#VID_093A&PID_2700#7&494a776&0&2#{a5dcbf10-6530-11d2-901f-00c04fb951ed}
Driver key name:  {36fc9e60-c465-11cf-8056-444553540000}\0045
Device instance ID:  USB\VID_093A&PID_2700\7&494A776&0&2
Device hardware ID:  USB\VID_093A&PID_2700&REV_0100
Device service:  usbccgp
Device friendly name:
Device location:  Port_#0002.Hub_#0006
Device physical object name:  \Device\USBPDO-5
| Device descriptor |
USB:  0x0200
Device class:  0xEF
Device subclass:  0x02
Device protocol:  0x01
Max packet size:  0x40 (64)
Vendor:  0x093A (Pixart Imaging, Inc.)
Product ID:  0x2700
Device ID:  0x0100
Manufacturer:  0x10 (PixArt Imaging Inc.)
Product:  0x60 (USB2.0_Camera)
Serial number ID:  0x00
Number of configurations:  1
Connection status:  Device connected
Current config value:  0x01
Device bus speed:  High (USB 2.0, 480 Mbit/s)
Device address:  0x06
Open pipes:   1
| Pipe information |
Endpoint address:  0x82, Input
Transfer type:  Interrupt
Max packet size:  0x0010 (16)
Interval:  0x06 (6)
| Configuration descriptor |
Total length:  0x02B5
Number of interfaces:  4
Configuration value:  0x01
Configuration:  0x30
Attributes:  0x80 (Bus powered)
Max power:  0xFA (500 Ma)
| Interface association descriptor |
First interface:  0x00
Interface count:  2
Function class:  0x0E
Function subclass:  0x03
Function protocol:  0x00
Function:  96
| Interface descriptor |
Interface number:  0x00

Alternate setting:  0x00
Num of endpoints:  1
Interface class:  0x0E (Video)
Interface subclass:  0x01 (Video Control)
Interface protocol ID:  0x00
Interface:  0x60 (USB2.0_Camera)
| Unknown descriptor |
Descriptor type:  0x24
Length:  0x0D (13)
0x0000:  0D 24 01 00 01 4D 00 C0 E1 E4 00 01 01
| Unknown descriptor |
Descriptor type:  0x24
Length:  0x09 (9)
0x0000:  09 24 03 02 01 01 00 04 00
| Unknown descriptor |
Descriptor type:  0x24
Length:  0x1A (26)
0x0000:  1A 24 06 04 F0 77 35 D1 89 8D 00 47 81 2E 7D D5
0x0010:  E2 FD B8 98 08 01 03 01 FF 00
| Unknown descriptor |
Descriptor type:  0x24
Length:  0x12 (18)
0x0000:  12 24 02 01 01 02 00 00 00 00 00 00 00 00 03 00
0x0010:  02 00
| Unknown descriptor |
Descriptor type:  0x24
Length:  0x0B (11)
0x0000:  0B 24 05 03 01 00 00 02 7F 05 00
| Endpoint descriptor |
Endpoint address:  0x82, Input
Transfer type:  Interrupt
Max packet size:  0x0010 (16)
Interval:  0x06 (6)
| Unknown descriptor |
Descriptor type:  0x25
Length:  0x05 (5)
0x0000:  05 25 03 10 00
| Interface descriptor |
Interface number:  0x01
Alternate setting:  0x00
Num of endpoints:  0
Interface class:  0x0E (Video)
Interface subclass:  0x02 (Video Streaming)
Interface protocol ID:  0x00
Interface ID:  0x00
| Unknown descriptor |
Descriptor type:  0x24
Length:  0x0E (14)
0x0000:  0E 24 01 01 43 01 81 00 02 02 01 00 01 00