Hub: 0 Port: 1                                                                                                                                              
DeviceClass: EF                                                                                                                                              
Vender: 046D                                                                                                                                              
Product: 0807                                                                                                                                              
InterfaceClass: 0E                                                                                                                                              
DESCRIPTOR_TYPE_CONFIGURATION                                                                                                                                              
NumInterfaces: 4                                                                                                                                              
DESCRIPTOR_TYPE_INTERFACE_ASSOCIATION                                                                                                                                              
FirstInterface: 0                                                                                                                                              InterfaceCount: 2                                                                                                                                              
FunctionClass: 0E                                                                                                                                              
FunctionSubClass: 03                                                                                                                                              FunctionProtocol: 00                                                                                                                                              Function: 0                                                                                                                                              DESCRIPTOR_TYPE_INTERFACE                                                                                                                                              InterfaceNumber: 0                                                                                                                                              AlternateSetting: 0                                                                                                                                              NumEndpoint: 1                                                                                                                                              InterfaceClass: 0E                                                                                                                                              InterfaceSubClass: 01                                                                                                                                              InterfaceProtocol: 00                                                                                                                                              Interface: 0                                                                                                                                              DESCRIPTOR_TYPE_CS_INTERFACE                                                                                                                                              CC_VIDEO                                                                                                                                              SC_VIDEOCONTROL                                                                                                                                              VC_HEADER                                                                                                                                              UVC: 0100                                                                                                                                              TotalLength: 217                                                                                                                                              ClockFrequency: 48000000                                                                                                                                              InCollection: 1                                                                                                                                              aInterfaceNr(1): 1                                                                                                                                              DESCRIPTOR_TYPE_CS_INTERFACE                                                                                                                                              CC_VIDEO                                                                                                                                              SC_VIDEOCONTROL                                                                                                                                              VC_INPUT_TERMINAL                                                                                                                                              TerminalID: 1                                                                                                                                              TerminalType: 0201                                                                                                                                              DESCRIPTOR_TYPE_CS_INTERFACE                                                                                                                                              CC_VIDEO                                                                                                                                              SC_VIDEOCONTROL                                                                                                                                              VC_PROCESSING_UNIT                                                                                                                                              UnitID: 2                                                                                                                                              SourceID: 1                                                                                                                                              MaxMultiplier: 16384                                                                                                                                              ControlSize: 2                                                                                                                                              Controls(1): 5B                                                                                                                                              Controls(2): 17                                                                                                                                              Processing: 0                                                                                                                                              VideoStanders: 1B                                                                                                                                              DESCRIPTOR_TYPE_CS_INTERFACE                                                                                                                                              CC_VIDEO                                                                                                                                              SC_VIDEOCONTROL                                                                                                                                              VC_EXTENSION_UNIT                                                                                                                                              UnitID: 4                                                                                                                                              DESCRIPTOR_TYPE_CS_INTERFACE                                                                                                                                              CC_VIDEO                                                                                                                                              SC_VIDEOCONTROL                                                                                                                                              VC_EXTENSION_UNIT                                                                                                                                              UnitID: 13                                                                                                                                              DESCRIPTOR_TYPE_CS_INTERFACE                                                                                                                                              CC_VIDEO                                                                                                                                              SC_VIDEOCONTROL                                                                                                                                              VC_EXTENSION_UNIT                                                                                                                                              UnitID: 8                                                                                                                                              DESCRIPTOR_TYPE_CS_INTERFACE                                                                                                                                              CC_VIDEO                                                                                                                                              SC_VIDEOCONTROL                                                                                                                                              VC_EXTENSION_UNIT                                                                                                                                              UnitID: 10                                                                                                                                              DESCRIPTOR_TYPE_CS_INTERFACE                                                                                                                                              CC_VIDEO                                                                                                                                              SC_VIDEOCONTROL                                                                                                                                              VC_EXTENSION_UNIT                                                                                                                                              UnitID: 14                                                                                                                                              DESCRIPTOR_TYPE_CS_INTERFACE                                                                                                                                              CC_VIDEO                                                                                                                                              SC_VIDEOCONTROL                                                                                                                                              VC_EXTENSION_UNIT                                                                                                                                              UnitID: 12                                                                                                                                              DESCRIPTOR_TYPE_CS_INTERFACE                                                                                                                                              CC_VIDEO                                                                                                                                              SC_VIDEOCONTROL                                                                                                                                              VC_OUTPUT_TERMINAL                                                                                                                                              TerminalID: 5                                                                                                                                              TerminalType: 0101                                                                                                                                              AssocTerminal: 0                                                                                                                                              SourceID: 4                                                                                                                                              Terminal: 0                                                                                                                                              DESCRIPTOR_TYPE_ENDPOINT                                                                                                                                              EndpointAddress: 87                                                                                                                                              Attributes: 03                                                                                                                                              MaxPacketSize: 16                                                                                                                                              Interval: 16                                                                                                                                              DESCRIPTOR_TYPE_INTERFACE                                                                                                                                              InterfaceNumber: 1                                                                                                                                              AlternateSetting: 0                                                                                                                                              NumEndpoint: 0                                                                                                                                              InterfaceClass: 0E                                                                                                                                              InterfaceSubClass: 02                                                                                                                                              InterfaceProtocol: 00                                                                                                                                              Interface: 0                                                                                                                                              DESCRIPTOR_TYPE_CS_INTERFACE                                                                                                                                              CC_VIDEO                                                                                                                                              SC_VIDEOSTREAMING                                                                                                                                              VS_INPUT_HEADER                                                                                                                                              NumFormats: 3                                                                                                                                              TotalLength: 592                                                                                                                                              EndpointAddress: 81                                                                                                                                              Info: 00                                                                                                                                              TerminalLink: 5                                                                                                                                              StillCaptureMethod: 2                                                                                                                                              TriggerSupport: 1                                                                                                                                              TriggerUsage: 0                                                                                                                                              ControlSize: 1                                                                                                                                              Controls(1): 00                                                                                                                                              DESCRIPTOR_TYPE_CS_INTERFACE                                                                                                                                              CC_VIDEO                                                                                                                                              SC_VIDEOSTREAMING                                                                                                                                              VS_FORMAT_UNCOMPRESSED                                                                                                                                              DESCRIPTOR_TYPE_CS_INTERFACE                                                                                                                                              CC_VIDEO                                                                                                                                              SC_VIDEOSTREAMING                                                                                                                                              VS_FRAME_UNCOMPRESSED                                                                                                                                              DESCRIPTOR_TYPE_CS_INTERFACE                                                                                                                                              CC_VIDEO                                                                                                                                              SC_VIDEOSTREAMING                                                                                                                                              VS_FRAME_UNCOMPRESSED                                                                                                                                              DESCRIPTOR_TYPE_CS_INTERFACE                                                                                                                                              CC_VIDEO                                                                                                                                              SC_VIDEOSTREAMING                                                                                                                                              VS_STILL_FRAME                                                                                                                                              EndpointAdress: 00                                                                                                                                              NumImageSizePatterns: 3                                                                                                                                              Width(1): 640                                                                                                                                              Height(1): 480                                                                                                                                              Width(2): 160                                                                                                                                              Height(2): 120                                                                                                                                              Width(3): 176                                                                                                                                              Height(3): 144                                                                                                                                              NumCompressPtn: 1                                                                                                                                              Compress(1): 5                                                                                                                                              DESCRIPTOR_TYPE_CS_INTERFACE                                                                                                                                              CC_VIDEO                                                                                                                                              SC_VIDEOSTREAMING                                                                                                                                              VS_COLOR_FORMAT                                                                                                                                              DESCRIPTOR_TYPE_CS_INTERFACE                                                                                                                                              CC_VIDEO                                                                                                                                              SC_VIDEOSTREAMING                                                                                                                                              VS_FORMAT_MJPEG                                                                                                                                              FormatIndex: 2                                                                                                                                              NumFrameDescriptors: 8                                                                                                                                              Flags: 1                                                                                                                                              DefaultFrameIndex: 1                                                                                                                                              DESCRIPTOR_TYPE_CS_INTERFACE                                                                                                                                              CC_VIDEO                                                                                                                                              SC_VIDEOSTREAMING                                                                                                                                              VS_FRAME_MJPEG                                                                                                                                              FrameIndex: 1                                                                                                                                              Capabilites: 0                                                                                                                                              Width: 640                                                                                                                                              Height: 480                                                                                                                                              MinBitRate: 24576000                                                                                                                                              MaxBitRate: 147456000                                                                                                                                              MaxVideoFrameBufferSize: 614400                                                                                                                                              DefaultFrameInterval: 333333                                                                                                                                              FrameIntervalType: 6                                                                                                                                              FrameInterval(1): 333333 (30.0 fps)                                                                         FrameInterval(2): 400000 (25.0 fps)                                                                         FrameInterval(3): 500000 (20.0 fps)                                                                         FrameInterval(4): 666666 (15.0 fps)                                                                         FrameInterval(5): 1000000 (10.0 fps)                                                                         FrameInterval(6): 2000000 (5.0 fps)                                                                         DESCRIPTOR_TYPE_CS_INTERFACE                                                                         CC_VIDEO                                                                         SC_VIDEOSTREAMING                                                                         VS_FRAME_MJPEG                                                                         FrameIndex: 2                                                                         Capabilites: 0                                                                         Width: 160                                                                         Height: 120                                                                         MinBitRate: 1536000                                                                         MaxBitRate: 9216000                                                                         MaxVideoFrameBufferSize: 38400                                                                         DefaultFrameInterval: 333333                                                                         FrameIntervalType: 6                                                                         FrameInterval(1): 333333 (30.0 fps)                                                                         FrameInterval(2): 400000 (25.0 fps)                                                                         FrameInterval(3): 500000 (20.0 fps)                                                                         FrameInterval(4): 666666 (15.0 fps)                                                                         FrameInterval(5): 1000000 (10.0 fps)                                                                         FrameInterval(6): 2000000 (5.0 fps)                                                                         DESCRIPTOR_TYPE_CS_INTERFACE                                                                         CC_VIDEO                                                                         SC_VIDEOSTREAMING                                                                         VS_FRAME_MJPEG                                                                         FrameIndex: 3                                                                         Capabilites: 0                                                                         Width: 176                                                                         Height: 144                                                                         MinBitRate: 2027520                                                                         MaxBitRate: 12165120                                                                         MaxVideoFrameBufferSize: 50688                                                                         DefaultFrameInterval: 333333                                                                         FrameIntervalType: 6                                                                         FrameInterval(1): 333333 (30.0 fps)                                                                         FrameInterval(2): 400000 (25.0 fps)                                                                         FrameInterval(3): 500000 (20.0 fps)                                                                         FrameInterval(4): 666666 (15.0 fps)                                                                         FrameInterval(5): 1000000 (10.0 fps)                                                                         FrameInterval(6): 2000000 (5.0 fps)                                                                         DESCRIPTOR_TYPE_CS_INTERFACE                                                                         CC_VIDEO                                                                         SC_VIDEOSTREAMING                                                                         VS_FRAME_MJPEG                                                                         FrameIndex: 4                                                                         Capabilites: 0                                                                         Width: 320                                                                         Height: 240                                                                         MinBitRate: 6144000                                                                         MaxBitRate: 36864000                                                                         MaxVideoFrameBufferSize: 153600                                                                         DefaultFrameInterval: 333333                                                                         FrameIntervalType: 6                                                                         FrameInterval(1): 333333 (30.0 fps)                                                                         FrameInterval(2): 400000 (25.0 fps)                                                                         FrameInterval(3): 500000 (20.0 fps)                                                                         FrameInterval(4): 666666 (15.0 fps)                                                                         FrameInterval(5): 1000000 (10.0 fps)                                                                         FrameInterval(6): 2000000 (5.0 fps)                                                                         DESCRIPTOR_TYPE_CS_INTERFACE                                                                         CC_VIDEO                                                                         SC_VIDEOSTREAMING                                                                         VS_FRAME_MJPEG                                                                         FrameIndex: 5                                                                         Capabilites: 0                                                                         Width: 352                                                                         Height: 288                                                                         MinBitRate: 8110080                                                                         MaxBitRate: 48660480                                                                         MaxVideoFrameBufferSize: 202752                                                                         DefaultFrameInterval: 333333                                                                         FrameIntervalType: 6                                                                         FrameInterval(1): 333333 (30.0 fps)                                                                         FrameInterval(2): 400000 (25.0 fps)                                                                         FrameInterval(3): 500000 (20.0 fps)                                                                         FrameInterval(4): 666666 (15.0 fps)                                                                         FrameInterval(5): 1000000 (10.0 fps)                                                                         FrameInterval(6): 2000000 (5.0 fps)                                                                         DESCRIPTOR_TYPE_CS_INTERFACE                                                                         CC_VIDEO                                                                         SC_VIDEOSTREAMING                                                                         VS_FRAME_MJPEG                                                                         FrameIndex: 6                                                                         Capabilites: 0                                                                         Width: 640                                                                         Height: 360                                                                         MinBitRate: 18432000                                                                         MaxBitRate: 110592000                                                                         MaxVideoFrameBufferSize: 460800                                                                         DefaultFrameInterval: 333333                                                                         FrameIntervalType: 6                                                                         FrameInterval(1): 333333 (30.0 fps)                                                                         FrameInterval(2): 400000 (25.0 fps)                                                                         FrameInterval(3): 500000 (20.0 fps)                                                                         FrameInterval(4): 666666 (15.0 fps)                                                                         FrameInterval(5): 1000000 (10.0 fps)                                                                         FrameInterval(6): 2000000 (5.0 fps)                                                                         DESCRIPTOR_TYPE_CS_INTERFACE                                                                         CC_VIDEO                                                                         SC_VIDEOSTREAMING                                                                         VS_FRAME_MJPEG                                                                         FrameIndex: 7                                                                         Capabilites: 0                                                                         Width: 640                                                                         Height: 400                                                                         MinBitRate: 20480000                                                                         MaxBitRate: 122880000                                                                         MaxVideoFrameBufferSize: 512000                                                                         DefaultFrameInterval: 333333                                                                         FrameIntervalType: 6                                                                         FrameInterval(1): 333333 (30.0 fps)                                                                         FrameInterval(2): 400000 (25.0 fps)                                                                         FrameInterval(3): 500000 (20.0 fps)                                                                         FrameInterval(4): 666666 (15.0 fps)                                                                         FrameInterval(5): 1000000 (10.0 fps)                                                                         FrameInterval(6): 2000000 (5.0 fps)                                                                         DESCRIPTOR_TYPE_CS_INTERFACE                                                                         CC_VIDEO                                                                         SC_VIDEOSTREAMING                                                                         VS_FRAME_MJPEG                                                                         FrameIndex: 8                                                                         Capabilites: 0                                                                         Width: 800                                                                         Height: 600                                                                         MinBitRate: 38400000                                                                         MaxBitRate: 115200000                                                                         MaxVideoFrameBufferSize: 960000                                                                         DefaultFrameInterval: 666666                                                                         FrameIntervalType: 3                                                                         FrameInterval(1): 666666 (15.0 fps)                                                                         FrameInterval(2): 1000000 (10.0 fps)                                                                         FrameInterval(3): 2000000 (5.0 fps)                                                                         DESCRIPTOR_TYPE_CS_INTERFACE                                                                         CC_VIDEO                                                                         SC_VIDEOSTREAMING                                                                         VS_STILL_FRAME                                                                         EndpointAdress: 00                                                                         NumImageSizePatterns: 8                                                                         Width(1): 640                                                                         Height(1): 480                                                                         Width(2): 160                                                                         Height(2): 120                                                                         Width(3): 176                                                                         Height(3): 144                                                                         Width(4): 320                                                                         Height(4): 240                                                                         Width(5): 352                                                                         Height(5): 288                                                                         Width(6): 640                                                                         Height(6): 360                                                                         Width(7): 640                                                                         Height(7): 400                                                                         Width(8): 800                                                                         Height(8): 600                                                                         NumCompressPtn: 5                                                                         Compress(1): 5                                                                         Compress(2): 10                                                                         Compress(3): 15                                                                         Compress(4): 20                                                                         Compress(5): 25                                                                         DESCRIPTOR_TYPE_CS_INTERFACE                                                                         CC_VIDEO                                                                         SC_VIDEOSTREAMING                                                                         VS_COLOR_FORMAT                                                                         DESCRIPTOR_TYPE_INTERFACE                                                                         InterfaceNumber: 1                                                                         AlternateSetting: 1                                                                         NumEndpoint: 1                                                                         InterfaceClass: 0E                                                                         InterfaceSubClass: 02                                                                         InterfaceProtocol: 00                                                                         Interface: 0                                                                         DESCRIPTOR_TYPE_ENDPOINT                                                                         EndpointAddress: 81                                                                         Attributes: 05                                                                         MaxPacketSize: 192                                                                         Interval: 1                                                                         DESCRIPTOR_TYPE_INTERFACE                                                                         InterfaceNumber: 1                                                                         AlternateSetting: 2                                                                         NumEndpoint: 1                                                                         InterfaceClass: 0E                                                                         InterfaceSubClass: 02                                                                         InterfaceProtocol: 00                                                                         Interface: 0                                                                         DESCRIPTOR_TYPE_ENDPOINT                                                                         EndpointAddress: 81                                                                         Attributes: 05                                                                         MaxPacketSize: 384                                                                         Interval: 1                                                                         DESCRIPTOR_TYPE_INTERFACE                                                                         InterfaceNumber: 1                                                                         AlternateSetting: 3                                                                         NumEndpoint: 1                                                                         InterfaceClass: 0E                                                                         InterfaceSubClass: 02                                                                         InterfaceProtocol: 00                                                                         Interface: 0                                                                         DESCRIPTOR_TYPE_ENDPOINT                                                                         EndpointAddress: 81                                                                         Attributes: 05                                                                         MaxPacketSize: 512                                                                         Interval: 1                                                                         DESCRIPTOR_TYPE_INTERFACE                                                                         InterfaceNumber: 1                                                                         AlternateSetting: 4                                                                         NumEndpoint: 1                                                                         InterfaceClass: 0E                                                                         InterfaceSubClass: 02                                                                         InterfaceProtocol: 00                                                                         Interface: 0                                                                         DESCRIPTOR_TYPE_ENDPOINT                                                                         EndpointAddress: 81                                                                         Attributes: 05                                                                         MaxPacketSize: 640                                                                         Interval: 1                                                                         DESCRIPTOR_TYPE_INTERFACE                                                                         InterfaceNumber: 1                                                                         AlternateSetting: 5                                                                         NumEndpoint: 1                                                                         InterfaceClass: 0E                                                                         InterfaceSubClass: 02                                                                         InterfaceProtocol: 00                                                                         Interface: 0                                                                         DESCRIPTOR_TYPE_ENDPOINT                                                                         EndpointAddress: 81                                                                         Attributes: 05                                                                         MaxPacketSize: 800                                                                         Interval: 1                                                                         DESCRIPTOR_TYPE_INTERFACE                                                                         InterfaceNumber: 1                                                                         AlternateSetting: 6                                                                         NumEndpoint: 1                                                                         InterfaceClass: 0E                                                                         InterfaceSubClass: 02                                                                         InterfaceProtocol: 00                                                                         Interface: 0                                                                         DESCRIPTOR_TYPE_ENDPOINT                                                                         EndpointAddress: 81                                                                         Attributes: 05                                                                         MaxPacketSize: 944                                                                         Interval: 1                                                                         DESCRIPTOR_TYPE_INTERFACE_ASSOCIATION                                                                         FirstInterface: 2                                                                         InterfaceCount: 2                                                                         FunctionClass: 01                                                                         FunctionSubClass: 02                                                                         FunctionProtocol: 00                                                                         Function: 0                                                                         DESCRIPTOR_TYPE_INTERFACE                                                                         InterfaceNumber: 2                                                                         AlternateSetting: 0                                                                         NumEndpoint: 0                                                                         InterfaceClass: 01                                                                         InterfaceSubClass: 01                                                                         InterfaceProtocol: 00                                                                         Interface: 0                                                                         DESCRIPTOR_TYPE_CS_INTERFACE                                                                         DESCRIPTOR_TYPE_CS_INTERFACE                                                                         DESCRIPTOR_TYPE_CS_INTERFACE                                                                         DESCRIPTOR_TYPE_CS_INTERFACE                                                                         DESCRIPTOR_TYPE_INTERFACE                                                                         InterfaceNumber: 3                                                                         AlternateSetting: 0                                                                         NumEndpoint: 0                                                                         InterfaceClass: 01                                                                         InterfaceSubClass: 02                                                                         InterfaceProtocol: 00                                                                         Interface: 0                                                                         DESCRIPTOR_TYPE_INTERFACE.InterfaceNumber: 3                                                                         AlternateSetting: 1                                                                         NumEndpoint: 1                                                                         InterfaceClass: 01                                                                         InterfaceSubClass: 02                                                                         InterfaceProtocol: 00                                                                         Interface: 0                                                                         DESCRIPTOR_TYPE_CS_INTERFACE                                                                         DESCRIPTOR_TYPE_CS_INTERFACE                                                                         DESCRIPTOR_TYPE_ENDPOINT                                                                         EndpointAddress: 86                                                                         Attributes: 05                                                                         MaxPacketSize: 68                                                                         Interval: 1                                                                         ..void uvc::_config(stcamcfg *)@321 cfg->FormatIndex == 1 ASSERT!