USB device details
Logitech, Inc. - Dispositivo compuesto USB

File:  \??\USB#VID_046D&PID_0807#016A6B60#{a5dcbf10-6530-11d2-901f-00c04fb951ed}
Driver key name:  {36fc9e60-c465-11cf-8056-444553540000}\0049
Device instance ID:  USB\VID_046D&PID_0807\016A6B60
Device hardware ID:  USB\VID_046D&PID_0807&REV_0009
Device service:  usbccgp
Device friendly name:
Device location:  Port_#0006.Hub_#0004
Device physical object name:  \Device\USBPDO-10
| Device descriptor |
USB:  0x0200
Device class:  0xEF
Device subclass:  0x02
Device protocol:  0x01
Max packet size:  0x40 (64)
Vendor:  0x046D (Logitech, Inc.)
Product ID:  0x0807
Device ID:  0x0009
Manufacturer:  0x00 (Logitech, Inc.)
Product ID:  0x00
Serial number:  0x02 (016A6B60)
Number of configurations:  1
Connection status:  Device connected
Current config value:  0x01
Device bus speed:  High (USB 2.0, 480 Mbit/s)
Device address:  0x02
Open pipes:   2
| Pipe information |
Endpoint address:  0x87, Input
Transfer type:  Interrupt
Max packet size:  0x0010 (16)
Interval:  0x08 (8)
| Pipe information |
Endpoint address:  0x81, Input
Transfer type:  Isochronous
Synchronization type:  asynchronous
Usage type:  data endpoint
Max packet size:  0x13FC (5116)
Interval:  0x01 (1)
| Configuration descriptor |
Total length:  0x07A1
Number of interfaces:  4
Configuration value:  0x01
Configuration ID:  0x00
Attributes:  0x80 (Bus powered)
Max power:  0xFA (500 Ma)
| Interface association descriptor |
First interface:  0x00

Interface count:  2
Function class:  0x0E
Function subclass:  0x03
Function protocol:  0x00
Function:  0
| Interface descriptor |
Interface number:  0x00
Alternate setting:  0x00
Num of endpoints:  1
Interface class:  0x0E (Video)
Interface subclass:  0x01 (Video Control)
Interface protocol ID:  0x00
Interface ID:  0x00
| Unknown descriptor |
Descriptor type:  0x24
Length:  0x0D (13)
0x0000:  0D 24 01 00 01 D9 00 00 6C DC 02 01 01
| Unknown descriptor |
Descriptor type:  0x24
Length:  0x12 (18)
0x0000:  12 24 02 01 01 02 00 00 00 00 00 00 00 00 03 0E
0x0010:  00 04
| Unknown descriptor |
Descriptor type:  0x24
Length:  0x0B (11)
0x0000:  0B 24 05 02 01 00 40 02 5B 17 00
| Unknown descriptor |
Descriptor type:  0x24
Length:  0x1B (27)
0x0000:  1B 24 06 04 82 06 61 63 70 50 AB 49 B8 CC B3 85
0x0010:  5E 8D 22 1E 0A 01 02 02 FF 03 00
| Unknown descriptor |
Descriptor type:  0x24
Length:  0x1B (27)
0x0000:  1B 24 06 0D 82 06 61 63 70 50 AB 49 B8 CC B3 85
0x0010:  5E 8D 22 1F 07 01 02 02 6F 01 00
| Unknown descriptor |
Descriptor type:  0x24
Length:  0x1C (28)
0x0000:  1C 24 06 08 82 06 61 63 70 50 AB 49 B8 CC B3 85
0x0010:  5E 8D 22 51 03 01 04 03 19 00 00 00
| Unknown descriptor |
Descriptor type:  0x24
Length:  0x1C (28)
0x0000:  1C 24 06 0A 82 06 61 63 70 50 AB 49 B8 CC B3 85
0x0010:  5E 8D 22 52 18 01 04 03 FF FF FF 00
| Unknown descriptor |
Descriptor type:  0x24
Length:  0x1C (28)